Feature  
Mini Ultra Thin contracted type structure  
Chocolate Keyboard  
Never get stuck.  
Brand new ABS plastic, Antibacterial and durable of keyboard  
≥ 10 Million tims  
> Waterproof keyboard with no sound and Elegant design  
It's accurate key system and quick in action of the key when touch  
with Chocolate key feel more comfortable  
MECHANICAL SPECIFICATIONS  
ELECTRICAL SPECIFICATIONS  
Total travel:3.0 + 0.4mm  
Insulation resistance: 100m OHM at 10.  
Initial actuating force: 25cn min  
Contact bounce: 5ms mar  
Operating force : 55 + 5cn  
Operation voltage: #5V DC  
Function: Normally open contact  
Operation current: 250mAma

Feature  
Mini Ultra Thin contracted type structure  
Chocolate Keyboard  
Never get stuck.  
Brand new ABS plastic, Antibacterial and durable of keyboard  
≥ 10 Million tims  
> Waterproof keyboard with no sound and Elegant design  
It's accurate key system and quick in action of the key when touch  
with Chocolate key feel more comfortable  
MECHANICAL SPECIFICATIONS  
ELECTRICAL SPECIFICATIONS  
Total travel:3.0 + 0.4mm  
Insulation resistance: 100m OHM at 10.  
Initial actuating force: 25cn min  
Contact bounce: 5ms mar  
Operating force : 55 + 5cn  
Operation voltage: #5V DC  
Function: Normally open contact  
Operation current: 250mAma

alx  
Software  
Engineering  
CERTIFICATE OF COMPLETION  
This is awarded to  
Abiola Oladunjoye  
For completing a 12 Month ALX Software Engineering  
Programme with a specialization in Back-end.  
FRED SWANIKER  
JULIEN BARBIER  
Founder & CEO, AL Group  
Chief Product Officer, ALX  
Date of Issue: 30th November 2023 POWERED BY Holberton Inc  
Scan the qr code or visit https://intranetalxswe com/certificates/Nc TERBBPGs to validate the certificate